DS-2CE56C0T-IT3

HD720P EXIR Turret Camera



**Key Features**

1 Megapixel high-performance CMOS

Analog HD output, up to 720P resolution

True Day/Night

DNR, Smart IR

EXIR technology, up to 40m IR distance

IP66 weatherproof

|  |  |  |
| --- | --- | --- |
|  |  | **Specifications** |
|  |  |  |
|  | ***Camera*** |  |
|  |  |  |
|  | Image Sensor | 1MP CMOS Image Sensor |
|  |  |  |
|  | Signal System | PAL/NTSC |
|  |  |  |
|  | Effective Pixels | 1296(H)\*732(V) |
|  |  |  |
|  | Min. illumination | 0.1 Lux @ (F1.2,AGC ON),0 Lux with IR |
|  |  |  |
|  | Shutter Time | 1/25(1/30)s to 1/50,000s |
|  |  |  |
|  | Lens | 3.6mm (2.8mm, 6mm, 8mm, 12mm, 16mm optional) |
|  |  |
|  | Angle of View: 70.9°(3.6mm), 92°(2.8mm), 56.7°(6mm), 38.6°(8mm), 27.5°(12mm), 17.7°(16mm) |
|  |  |
|  |  |  |
|  | Lens Mount | M12 |
|  |  |  |
|  | Day & Night | ICR |
|  |  |  |
|  | Angle Adjustment | Pan: 0 - 360°, Tilt: 0 - 75°, Rotation: 0 - 360° |
|  |  |  |
|  | Synchronization | Internal synchronization |
|  |  |  |
|  | Video Frame Rate | 720p@25fps/720p@30fps |
|  |  |  |
|  | HD Video Output | 1 Analog HD output |
|  |  |  |
|  | S/N Ratio | ＞62dB |
|  | ***General*** |  |
|  |  |  |
|  | Operating Conditions | -40 °C – 60 °C (-40 °F – 140 °F), Humidity 90% or less (non-condensing) |
|  |  |  |
|  | Power Supply | 12 VDC±15% |
|  |  |  |
|  | Power Consumption | Max. 4W |
|  |  |  |
|  | Protection Level | IP66 |
|  |  |  |
|  | IR Range | Up to 40m |
|  |  |  |
|  | Dimensions | Φ110 × 93.2 mm(Φ4.33” × 3.67”) |
|  |  |  |
|  | Weight | 350 g |
|  |  |  |